{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A9"]
[]
[]
[]
[]
["","","","","","4MXM80A2V1B9"]
["Dimensions","Unit","","Height","mm","734"]
["","","","Width","mm","974"]
["","","","Depth","mm","408"]
["Weight","Unit","","","kg","67"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","49"]
["Refrigerant","Type","","","","R-32"]
["","Charge","","","kg","2.4"]
["","Charge","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","25 (1)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Total piping length","System","Actual","m","70"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain cap (1)","","","","6"]
["","Drain cap (2)","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Power supply","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]
["Notes","","","","","(1) - For one room"]