{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N9"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B9"]
["Refrigerant","Charge","","","kg","2"]
["Sound pressure level","Heating","","Nom.","dB(A)","49.0"]
["","Cooling","","Nom.","dB(A)","48"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5"]
["","Total piping length","System","Actual","m","60"]
["","Piping length","OU - IU","Max.","m","25 (1)"]
["Dimensions","Unit","","Depth","mm","340"]
["Weight","Unit","","","kg","63"]
["Dimensions","Unit","","Width","mm","958"]
["","","","Height","mm","734"]
["Refrigerant","Charge","","","tCO2Eq","1.35"]
["Piping connections","Level difference","IU - OU","Max.","m","15.0"]
["Operation range","Cooling","Ambient","Max.","°CDB","46"]
["","","","Min.","°CDB","-10"]
["Fan motor","Speed","Cooling","Super low","rpm","420"]
["","","Heating","Super low","rpm","420"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain cap (1)","","","","6"]
["","Drain cap (2)","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - For one room"]