{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA50A2VEB","ADEA100A2VEB"]
["Fan","External static pressure","","High","Pa","","150"]
["Casing","Colour","","","","","Not painted (galvanised)"]
["","Material","","","","","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","","245"]
["","","","Width","mm","","1400"]
["","","","Depth","mm","","800"]
["Weight","Unit","","","kg","","46"]
["Fan","Air flow rate","Cooling","High","m³/min","","29"]
["","","","Medium","m³/min","","26"]
["","","","Low","m³/min","","23"]
["","","Heating","High","m³/min","","29"]
["","","","Medium","m³/min","","26"]
["","","","Low","m³/min","","23"]
["","External static pressure","","Nom.","Pa","","40"]
["Sound power level","Cooling","","","dBA","","58"]
["Sound pressure level","Cooling","","High","dBA","","34"]
["","","","Medium","dBA","","32"]
["","","","Low","dBA","","30"]
["","Heating","","High","dBA","","36"]
["","","","Medium","dBA","","33"]
["","","","Low","dBA","","30"]
["Piping connections","Liquid","","OD","mm","","9.52"]
["","Gas","","OD","mm","","15.9"]
["","Drain","","","","","VP20 (I.D. 20/O.D. 26)"]
["Drain-up height","mm","","","","","625"]
["Control systems","Infrared remote control","","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","","1"]
["","Washer for hanger bracket","","","","","8"]
["","Operation manual","","","","","1"]
["","Clamps","","","","","4"]
["","Drain hose","","","","","1"]
["","Insulation for fitting","","","","","2"]
["","Metal clamp for drain hose","","","","","1"]
["","Screws","","","","","40"]
["","Sealing pads","","","","","5"]
["Power supply","Phase","","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","","50"]
["","Power supply-=-Voltage","","Voltage","","","220-240/220"]
["Standard Accessories","AAA dry-cell batteries","","","","3"]