{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A / EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA / EJHA04AAV3"]
["Heating capacity","Nom.","","","kW","3.83 (1)"]
["","Max.","","","kW","4.53 (1)"]
["Power input","Heating","","Min.","kW","0.850 (1)"]
["","","","Nom.","kW","1.07 (1)"]
["COP","","","","","4.49 (1)"]
["Pump","ESP","Heating","Min","kPa","25.0 (4)"]
["","","","Max","kPa","45.0 (4)"]
["Domestic hot water heating","General","","Declared load profile","","XL"]
["","Average climate","","Water heating energy efficiency class","","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.26"]
["","","","Seasonal space heating eff. class","","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","128"]
["","Average climate water outlet 35°C","General","SCOP","","4.14"]
["","","","ηs (Seasonal space heating efficiency)","%","163"]
["","","","Seasonal space heating eff. class","","A++"]
["Notes","","","","","(1) - Heating: leaving condenser water temp. 35°C; Dt 5°C; ambient air temp. 7°CDB, 6°CWB"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), boiler bypassed"]
["","","","","","(4) - Depends upon the length of field pipe"]