{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EJHA04AAV3"]
["Heating capacity","Nom.","","","kW","4.53"]
["Power input","Heating","","Nom.","kW","0.850"]
["COP","","","","","4.49"]
["Dimensions","Unit","","Height","mm","745"]
["","","","Width","mm","845"]
["","","","Depth","mm","329"]
["Weight","Unit","","","kg","45.0"]
["Fan","Air flow rate","Heating","High","m³/min","28.3"]
["Operation range","Heating","Ambient","Max.","°CWB","25"]
["","Domestic hot water","Ambient","Min.","°CDB","-14"]
["","","","Max.","°CDB","35"]
["Sound power level","Heating","","Nom.","dBA","58.7"]
["Sound pressure level","Heating","","Nom.","dBA","37.0"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","kg","0.560"]
["","Charge","","","tCO2Eq","0.380"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","2.60"]
["","","","Seasonal space heating eff. class","","A+"]
["","Average climate water outlet 35°C","General","SCOP","","2.98"]
["","","","Seasonal space heating eff. class","","A"]
["Power supply","Name","","","","V3"]
["","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]
["Notes","","","","","(1) - Heating: leaving condenser water temp. 35°C; Dt 5°C; ambient air temp. 7°CDB, 6°CWB"]