{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWSAH-UD9W"]
[]
[]
[]
[]
["","","","","","EWSAH06UDA9W"]
["Space heating","Average climate water outlet 35°C","General","Seasonal space heating eff. class","","A+++"]
["","","","SCOP","","6.49"]
["Refrigerant","GWP","","","","675.0"]
["Casing","Colour","","","","White + Black"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","4.15"]
["Casing","Material","","","","Precoated sheet metal"]
["Refrigerant","Type","","","","R-32"]
["Weight","Unit","","","kg","222"]
["Tank","Corrosion protection","","","","Pickling"]
["Space heating","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A+++"]
["Refrigerant","Charge","","","kg","1.70"]
["Tank","Insulation","","Heat loss","kWh/24h","1.4"]
["Dimensions","Unit","","Depth","mm","666"]
["Refrigerant","Charge","","","tCO2Eq","1.15"]
["Dimensions","Unit","","Width","mm","597"]
["","","","Height","mm","1891"]
["Tank","Water volume","","","l","180"]
["Power supply","Power supply-=-Voltage","","Voltage","","230/400"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Phase","","","","1~/3~"]
["Current","Current-=-Recommended fuses","","Recommended fuses","","16/32"]
["Notes","","","","","(1) - According to EN14825 and EN14511:2018"]