{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","","FCAHG71FVEB"]
["Casing","Material","","","","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","288"]
["","","","Width","mm","840"]
["","","","Depth","mm","840"]
["Weight","Unit","","","kg","25.0"]
["Fan","Air flow rate","Cooling","High","m³/min","21.2"]
["","","","Medium","m³/min","16.7"]
["","","","Low","m³/min","12.2"]
["","","Heating","High","m³/min","21.2"]
["","","","Medium","m³/min","16.7"]
["","","","Low","m³/min","12.2"]
["Sound power level","Cooling","","","dBA","53"]
["","Heating","","","dBA","53"]
["Sound pressure level","Cooling","","High","dBA","36"]
["","","","Medium","dBA","33"]
["","","","Low","dBA","29"]
["","Heating","","High","dBA","36"]
["","","","Medium","dBA","33"]
["","","","Low","dBA","29"]
["Refrigerant","GWP","","","","675"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)"]
["Decoration panel","Model","","","","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","130"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","10"]
["Decoration panel 2","Model","","","","BYCQ140D7GW1 - auto cleaning panel"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","130"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","10.3"]
["Decoration panel 3","Model","","","","BYCQ140D7W1W - full white, See note 1"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","50"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","5.4"]
["Decoration panel 4","Model","","","","BYCQ140D7W1 - white with grey louvers"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","50"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","5.4"]
["Standard Accessories","Installation manual","","","","Installation manual"]
["","Installation and operation manual","","","","Installation and operation manual"]
["Power supply","Name","","","","VE"]
["","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240"]