{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG71HVEB","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Piping connections","Liquid","","OD","mm","","","9.52"]
["Dimensions","Unit","","Width","mm","","","840"]
["","","","Height","mm","","","288"]
["","","","Depth","mm","","","840"]
["Weight","Unit","","","kg","","","25"]
["Fan","Air flow rate","Cooling","High","m³/min","","","34.4"]
["","","","Low","m³/min","","","21.2"]
["Decoration panel 3","Dimensions","","Depth","mm","","","950"]
["","Weight","","","kg","","","6.5"]
["","","","Width","mm","","","950"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10"]
["Decoration panel 3","Dimensions","","Height","mm","","","106"]
["Sound pressure level","Heating","","High","dBA","","","45"]
["","Cooling","","Low","dBA","","","35"]
["Piping connections","Gas","","OD","mm","","","15.9"]
["Fan","Air flow rate","Heating","Medium","m³/min","","","25.5"]
["Sound power level","Heating","","","dBA","","","61"]
["Fan","Air flow rate","Cooling","Medium","m³/min","","","27.3"]
["","","Heating","High","m³/min","","","32.1"]
["","","","Low","m³/min","","","19.7"]
["Sound pressure level","Cooling","","High","dBA","","","45"]
["","Heating","","Low","dBA","","","35"]
["","","","Medium","dBA","","","40"]
["Decoration panel","Weight","","","kg","","","5.5"]
["Sound pressure level","Heating","","Medium","dBA","","","40"]
["Sound power level","Cooling","","","dBA","","","61"]
["Heating capacity","Total capacity","","Nom.","kW","","","13.5"]
["Decoration panel 2","Dimensions","","Width","mm","","","950"]
["","","","Depth","mm","","","950"]
["","Weight","","","kg","","","10.3"]
["Decoration panel","Dimensions","","Depth","mm","","","950"]
["Decoration panel 2","Dimensions","","Height","mm","","","148"]
["Decoration panel","Dimensions","","Height","mm","","","65"]
["","","","Width","mm","","","950"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual","1","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket","Washer for hanger bracket","8","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual","Operation manual","1","Operation manual"]
["","Wire clamp material","","","","Wire clamp material","Wire clamp material","7","Wire clamp material"]
["","Clamp for drain hose","","","","Clamp for drain hose","Clamp for drain hose","1","Clamp for drain hose"]
["","Clamps","","","","Clamps","Clamps","1","Clamps"]
["","Drain hose","","","","Drain hose","Drain hose","1","Drain hose"]
["","Installation guide","","","","Installation guide","Installation guide","1","Installation guide"]
["","Insulation for fitting","","","","Insulation for fitting","Insulation for fitting","2","Insulation for fitting"]
["","Screws","","","","Screws","Screws","4","Screws"]
["","Sealing pads","","","","Sealing pads","Sealing pads","1","Sealing pads"]
["Casing","Material","","","","","","Galvanised steel plate"]
["Piping connections","Drain","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Decoration panel","Model","","","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["Decoration panel 2","Model","","","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["Decoration panel 3","Model","","","","","","BYCQ140E2P, BYCQ140E2PB"]
["Control systems","Infrared remote control","","","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["","Wired remote control","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Power supply","Phase","","","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","","","50/60"]
["","Power supply-=-Voltage","","Voltage","","","","220-240/220"]