{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS / RXJ-A"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BS / RXJ20A5V1B","FTXJ25A2V1BS / RXJ25A5V1B","FTXJ35A2V1BS / RXJ35A5V1B","FTXJ42A2V1BS / RXJ42A2V1B","FTXJ50A2V1BS / RXJ50A2V1B"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.40","1.70","1.70"]
["","Max.","","kW","2.60","3.20","4.00","5.00","5.30"]
["","Nom.","","kW","2.00","2.50","3.40","4.20","5.00"]
["Space cooling","SEER","","","8.75","8.74","8.73","7.50","7.33"]
["","Annual energy consumption","","kWh/a","80","100","136","196","239"]
["","Capacity","Pdesign","kW","2.00","2.50","3.40","4.20","5.00"]
["","Energy efficiency class","","","A+++","A+++","A+++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.45","2.50","3.80","4.00"]
["","SCOP/A","","","5.15","5.15","5.15","4.60","4.60"]
["","Energy efficiency class","","","A+++","A+++","A+++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.02","2.07","2.11","3.26","3.44"]
["","Annual energy consumption","","kWh/a","652","666","680","1,156","1,218"]
["Nominal efficiency","Annual energy consumption","","kWh","213","280","389","526","679"]
["","EER","","","4.70","4.46","4.37","3.99","3.68"]
["","COP","","","5.00","5.00","4.04","4.12","4.00"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.50","2.80","4.00","5.40","5.80"]
["","Min.","","kW","1.30","1.30","1.40","1.70","1.70"]
["","Max.","","kW","3.50","4.70","5.20","6.00","6.50"]
["Notes","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]