{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-N"]
[]
[]
[]
[]
["","","","","FTXJ50MV1BW / RXJ50N2V1B"]
["Cooling capacity","Min.","","kW","1.40"]
["","Max.","","kW","5.50"]
["","Nom.","","kW","4.80"]
["Space cooling","SEER","","","7.02"]
["","Annual energy consumption","","kWh/a","239"]
["","Capacity","Pdesign","kW","4.80"]
["","Energy efficiency class","","","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.60"]
["","SCOP/A","","","4.28"]
["","Energy efficiency class","","","A+"]
["","Pdh Heating capacity at -10°","","kW","4.09"]
["","Annual energy consumption","","kWh/a","1,505"]
["Nominal efficiency","Annual energy consumption","","kWh","716"]
["","EER","","","3.35"]
["","COP","","","3.65"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Heating capacity","Nom.","","kW","5.80"]
["","Min.","","kW","1.10"]
["","Max.","","kW","7.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data"]