{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM42M2V1B"]
["Power input","Cooling","","Nom.","kW","0.035"]
["","Heating","","Nom.","kW","0.035"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","294"]
["","","","Width","mm","811"]
["","","","Depth","mm","272"]
["Weight","Unit","","","kg","10"]
["Fan","Air flow rate","Cooling","High","m³/min","12.6"]
["","","","Medium","m³/min","9.5"]
["","","","Low","m³/min","7.1"]
["","","","Silent operation","m³/min","4.6"]
["","","Heating","High","m³/min","13"]
["","","","Medium","m³/min","10.4"]
["","","","Low","m³/min","7.1"]
["","","","Silent operation","m³/min","5.3"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","60"]
["Sound pressure level","Cooling","","High","dBA","45"]
["","","","Medium","dBA","39"]
["","","","Low","dBA","30"]
["","","","Silent operation","dBA","21"]
["","Heating","","High","dBA","45"]
["","","","Medium","dBA","39"]
["","","","Low","dBA","29"]
["","","","Silent operation","dBA","21"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","12.7"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]