{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M"]
[]
[]
[]
[]
["","","","","","FTXP20M5V1B","FTXP25M5V1B","FTXP35M5V1B","FTXP50M2V1B","FTXP60M2V1B"]
["Sound pressure level","Heating","","High","dBA","39","40","40","38","40"]
["","","","Medium","dBA","34","34","35","33","35"]
["","","","Silent operation","dBA","21","21","21"]
["","","","Low","dBA","28","28","29","30","32"]
["","Cooling","","Medium","dBA","33","33","34","39","41"]
["","","","Silent operation","dBA","19","19","20","27","30"]
["","","","Low","dBA","25","26","27","34","36"]
["","","","High","dBA","39","40","43","43","45"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53","ARC480A53","ARC480A53"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50","9.50","12.7","12.7"]
["","Drain","","","","18","18","18","18","18"]
["Power input","Cooling","","Nom.","kW","0.019","0.020","0.032","0.029","0.032"]
["","Heating","","Nom.","kW","0.023","0.023","0.032","0.032","0.035"]
["Sound power level","Cooling","","","dBA","55","55","58","59","60"]
["","Heating","","","dBA","55","55","58","61","62"]
["Dimensions","Unit","","Width","mm","770","770","770","990","990"]
["","","","Depth","mm","225","225","225","263","263"]
["","","","Height","mm","286","286","286","295","295"]
["Casing","Colour","","","","White","White","White","White","White"]
["Weight","Unit","","","kg","8.50","8.50","9.00","13.5","13.5"]
["Fan","Air flow rate","Heating","High","m³/min","10.4","10.4","11.5","17.3","17.9"]
["","","","Medium","m³/min","8.1","8.1","9.0","14.4","15.3"]
["","","","Low","m³/min","6.2","6.4","7.0","11.8","12.4"]
["","","","Silent operation","m³/min","5.2","5.2","5.3","10.4","11.0"]
["","","Cooling","Low","m³/min","5.6","5.8","6.3","11.5","11.8"]
["","","","Medium","m³/min","7.4","7.7","8.3","14.0","14.4"]
["","","","High","m³/min","9.5","9.7","11.5","16.3","16.8"]
["","","","Silent operation","m³/min","4.2","4.2","4.5","8.3","9.2"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~"]
["","Name","","","","","","","V1","V1"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Silver particle filter","","","","1","","","1","1"]