{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP25M5V1B9","FTXP35M5V1B9"]
["Sound pressure level","Heating","","High","dBA","40","40"]
["","","","Medium","dBA","34","35"]
["","","","Silent operation","dBA","21","21"]
["","","","Low","dBA","28","29"]
["","Cooling","","Medium","dBA","33","34"]
["","","","Silent operation","dBA","19","20"]
["","","","Low","dBA","26","27"]
["","","","High","dBA","40","43"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A53","ARC480A53"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50"]
["","Drain","","","","18","18"]
["Power input","Cooling","","Nom.","kW","0.020","0.032"]
["","Heating","","Nom.","kW","0.023","0.032"]
["Sound power level","Cooling","","","dBA","55","58"]
["","Heating","","","dBA","55","58"]
["Dimensions","Unit","","Width","mm","770","770"]
["","","","Depth","mm","225","225"]
["","","","Height","mm","286","286"]
["Casing","Colour","","","","White","White"]
["Weight","Unit","","","kg","8.50","9.00"]
["Fan","Air flow rate","Heating","High","m³/min","10.4","11.5"]
["","","","Medium","m³/min","8.1","9.0"]
["","","","Low","m³/min","6.4","7.0"]
["","","","Silent operation","m³/min","5.2","5.3"]
["","","Cooling","Low","m³/min","5.8","6.3"]
["","","","Medium","m³/min","7.7","8.3"]
["","","","High","m³/min","9.7","11.5"]
["","","","Silent operation","m³/min","4.2","4.5"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]