{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":12,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAA-A"]
[]
[]
[]
[]
["","","","","","FXAA25AUV1B","FXAA63AUV1B","FXAA50AUV1B","FXAA32AUV1B","FXAA20AUV1B","FXAA15AUV1B","FXAA40AUV1B"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","9.52","12.70","12.70","9.52","9.52","9.52","12.70"]
["","","","OD","mm","6","6","6","6","6","6","6"]
["","Gas","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.028","0.050","0.033","0.030","0.019","0.017","0.025"]
["Sound pressure level","Heating","","At low fan speed","dBA","28.5","38.5","35.5","28.5","28.5","28.5","33.5"]
["Piping connections","Drain","","","","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)"]
["Air filter","Type","","","","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable"]
["Fan","Air flow rate - 50Hz","Cooling","At low fan speed","m³/min","6.5","12.9","10.9","6.5","6.5","6.5","9.8"]
["","","","At high fan speed","m³/min","8.3","18.2","14.2","9.4","7.9","7.1","12.2"]
["Power input - 50Hz","Heating","","At high fan speed","kW","0.034","0.060","0.039","0.035","0.029","0.025","0.030"]
["Sound pressure level","Cooling","","At low fan speed","dBA","28.5","38.5","35.5","28.5","28.5","28.5","33.5"]
["","Heating","","At high fan speed","dBA","36.0","47.0","42.0","38.5","34.0","33.0","38.0"]
["","","","At medium fan speed","dBA","32.5","43.0","39.0","33.5","31.5","31.0","36.0"]
["","","","At medium fan speed","dBA","32.0","42.5","38.5","33.0","31.0","30.5","35.5"]
["","","","At high fan speed","dBA","35.0","46.5","41.0","37.5","33.0","32.0","37.0"]
["Sound power level","Cooling","","At high fan speed","dBA","53.0","63.0","58.0","55.0","52.0","51.0","55.0"]
["Casing","Colour","","","","White","White","White","White","White","White","White"]
["Weight","Unit","","","kg","12","15","15","12","12","12","15"]
["Dimensions","Unit","","Depth","mm","266","269","269","266","266","266","269"]
["","","","Width","mm","795","1050","1050","795","795","795","1050"]
["","","","Height","mm","290","290","290","290","290","290","290"]
["Heating capacity","Total capacity","","At high fan speed","kW","3.2","8.0","6.3","4.0","2.5","1.9","5.0"]
["Cooling capacity","Total capacity","","At high fan speed","kW","2.8","7.1","5.6","3.6","2.2","1.7","4.5"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Standard Accessories","Installation plate","","","","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","4","4","4","4","4","4","4"]
["","Heat insulating tape","","","","1","1","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1","1","1"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","6","6","6","6"]
["Power supply","Name","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Power supply-=-Frequency","","Frequency","","50","50","50","50","50","50","50"]
["","Power supply-=-Voltage","","Voltage","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]