{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Fan","Air flow rate","Air purifying operation","Low","m³/h","132"]
["","","Humidifying operation","Low","m³/h","132"]
["","","","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["Humidifying operation","Power input","","L","kW","0.012"]
["Air purifying operation","Power input","","Silent","kW","0.008"]
["Humidifying operation","Water tank capacity","","","l","3.6"]
["Air purifying operation","Power input","","M","kW","0.016"]
["Humidifying operation","Power input","","Silent","kW","0.011"]
["","","","M","kW","0.018"]
["Air purifying operation","Power input","","L","kW","0.010"]
["Humidifying operation","Power input","","Turbo","kW","0.068"]
["Application","","","","","Floor standing type"]
["Weight","Unit","","","kg","12.5"]
["Air purifying operation","Power input","","Turbo","kW","0.066"]
["Sound pressure level","Humidifying operation","","Silent","dBA","23"]
["Fan","Air flow rate","Air purifying operation","Silent","m³/h","60"]
["Sound pressure level","Humidifying operation","","Low","dBA","27"]
["","","","Turbo","dBA","54"]
["Applicable room area","m²","","","","48, 96"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","420"]
["Sound pressure level","Air purifying operation","","Silent","dBA","18"]
["","","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","Humidifying operation","","Medium","dBA","37"]
["","","","Low","dBA","27"]
["Fan","Air flow rate","Humidifying operation","Medium","m³/h","210"]
["","","","Silent","m³/h","102"]
["Casing","Colour","","","","White (N9. 0)"]
["Dimensions","Unit","","Depth","mm","287"]
["","","","Width","mm","395"]
["Type","","","","","Humidifying air purifier"]
["Dimensions","Unit","","Height","mm","600"]
["CADR","m³/h","","","","375"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Power supply","Power supply-=-Frequency","","Frequency","","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240/220-230"]
["","Phase","","","","1~"]
["Power cord","m","","","","2.0"]
["Notes","","","","","(1) - Converted to NRCC standards from test values in accordance with JEM1467."]
["","","","","","(2) - The coverage area is appropriate for operating the unit of maximum fan speed(HH). Coverage area indicates the space where a certain amount of dust particles can be removed in 30 minutes."]
["","","","","","(3) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]