{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B"]
["Dimensions","Unit","","Height","mm","990"]
["","","","Width","mm","940"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","67"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-15"]
["","","","Max.","°CDB","50"]
["","Heating","Ambient","Min.","°CWB","-20"]
["","","","Max.","°CWB","15.5"]
["Sound power level","Cooling","","","dBA","64"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","50"]
["","Night quiet mode","","Level 1","dBA","43"]
["Refrigerant","Type","","","","R-32"]
["","Charge","","","kg","2.6"]
["","GWP","","","","675"]
["","Charge","","","tCO2Eq","1.8"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Piping length","OU - IU","Max.","m","55"]
["","","System","Equivalent","m","75"]
["","","","Chargeless","m","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual"]
["","Level difference","IU - OU","Max.","m","30.0"]
["","","IU - IU","Max.","m","0.5"]
["Standard Accessories","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Power supply","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240"]