{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-A"]
[]
[]
[]
[]
["","","RXJ25A5V1B","RXJ35A5V1B","RXJ42A2V1B","RXJ50A2V1B"]
["Standard Accessories","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Refrigerant charge label","Refrigerant charge label","Refrigerant charge label","Refrigerant charge label","Refrigerant charge label"]
["","Multilingual fluorinated greenhouse gases labels","Multilingual fluorinated greenhouse gases labels","Multilingual fluorinated greenhouse gases labels","Multilingual fluorinated greenhouse gases labels","Multilingual fluorinated greenhouse gases labels"]
["","General safety precautions","General safety precautions","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain plug","Drain plug","Drain plug","Drain plug","Drain plug"]
["","Drain cap (1)","","","Drain cap (1)","Drain cap (1)"]
["","Drain cap (2)","","","Drain cap (2)","Drain cap (2)"]